#!/usr/bin/env bash
#
# Build tests for AT90USB1286 (DFU)
#

# exit on first failure
set -e

#
# Build with the default configurations
#
restore_configs
opt_set MOTHERBOARD BOARD_PRINTRBOARD
exec_test $1 $2 "Printrboard Configuration" "$3"

restore_configs
opt_set MOTHERBOARD BOARD_PRINTRBOARD_REVF
opt_enable MINIPANEL
exec_test $1 $2 "Printrboard RevF with MiniPanel and Stepper DAC (in pins file)" "$3"

# clean up
restore_configs
